[gd_scene load_steps=6 format=3 uid="uid://dnxq870xf6pkh"]

[ext_resource type="Texture2D" uid="uid://c4mdrmk7h638f" path="res://data/nine-patch-round.png" id="1_pfrxy"]
[ext_resource type="PackedScene" uid="uid://7ps8s0jd2bdr" path="res://scenes/контроль/блок-б.tscn" id="2_dmhrm"]
[ext_resource type="PackedScene" uid="uid://bkxblfoj7ejv0" path="res://scenes/контроль/блок-а.tscn" id="3_5ikxk"]
[ext_resource type="PackedScene" uid="uid://d3iqb5e4g81m5" path="res://scenes/контроль/элемент-г.tscn" id="4_mtf2n"]

[sub_resource type="GDScript" id="GDScript_y4aoq"]
script/source = "extends Control

signal pressed(control: PanelContainer)

func _on_item_pressed(control): emit_signal('pressed', control)
"

[node name="bort_afsp" type="Control"]
layout_mode = 3
anchors_preset = 0
offset_right = 580.0
offset_bottom = 1185.0
script = SubResource("GDScript_y4aoq")
metadata/DeviceName = &""
metadata/_edit_vertical_guides_ = [-1620.0]

[node name="konverter" type="NinePatchRect" parent="."]
layout_mode = 0
offset_top = 926.0
offset_right = 580.0
offset_bottom = 1190.0
texture = ExtResource("1_pfrxy")
patch_margin_left = 16
patch_margin_top = 16
patch_margin_right = 16
patch_margin_bottom = 16

[node name="lbl_fname" type="Label" parent="konverter"]
self_modulate = Color(1, 1, 1, 0.62)
layout_mode = 0
offset_left = 5.0
offset_top = 5.0
offset_right = 575.0
offset_bottom = 25.0
text = "Конвертер 1000...6000 МГц"
horizontal_alignment = 1
vertical_alignment = 1

[node name="grid" type="GridContainer" parent="konverter"]
layout_mode = 2
offset_left = 10.0
offset_top = 25.0
offset_right = 570.0
offset_bottom = 257.0
columns = 4

[node name="kanal1" parent="konverter/grid" instance=ExtResource("2_dmhrm")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Канал №1 конвертера 1000...6000 МГц"
value0 = 24.0
value1 = 10.0
min_value0 = 10.0
min_value1 = 15.0
max_value0 = 35.0
max_value1 = 30.0
step0 = 1.0
step1 = 1.0
value_name0 = "t, °C"
value_name1 = "U, В"
value_name2 = "CAN"
name_min_size0 = Vector2i(35, 20)
name_min_size1 = Vector2i(35, 20)
name_min_size2 = Vector2i(35, 20)
fname = "Канал 1"
metadata/value0 = "SelfTest[0].SystemList[1].DevList[0].TestedParamList[0]['CurrentValue']"
metadata/value1 = "SelfTest[0].SystemList[1].DevList[0].TestedParamList[0]['CurrentValue']"
metadata/value2 = "SelfTest[0].SystemList[1].DevList[0]['TestPassed']"
metadata/state = ["SelfTest[0].SystemList[1].DevList[0]['TestPassed']"]

[node name="kanal2" parent="konverter/grid" instance=ExtResource("2_dmhrm")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Канал №2 конвертера 1000...6000 МГц"
value0 = 24.0
value1 = 27.0
min_value0 = 10.0
min_value1 = 15.0
max_value0 = 35.0
max_value1 = 30.0
step0 = 1.0
step1 = 1.0
value_name0 = "t, °C"
value_name1 = "U, В"
value_name2 = "CAN"
name_min_size0 = Vector2i(35, 20)
name_min_size1 = Vector2i(35, 20)
name_min_size2 = Vector2i(35, 20)
fname = "Канал 2"
metadata/value0 = "SelfTest[1].SystemList[1].DevList[1].TestedParamList[0]['CurrentValue']"
metadata/value1 = "SelfTest[2].SystemList[1].DevList[1].TestedParamList[0]['CurrentValue']"
metadata/value2 = "SelfTest[0].SystemList[1].DevList[1]['TestPassed']"
metadata/state = ["SelfTest[0].SystemList[1].DevList[1]['TestPassed']"]

[node name="kanal3" parent="konverter/grid" instance=ExtResource("2_dmhrm")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Канал №3 конвертера 1000...6000 МГц"
value0 = 24.0
value1 = 27.0
min_value0 = 10.0
min_value1 = 15.0
max_value0 = 35.0
max_value1 = 30.0
step0 = 1.0
step1 = 1.0
value_name0 = "t, °C"
value_name1 = "U, В"
value_name2 = "CAN"
name_min_size0 = Vector2i(35, 20)
name_min_size1 = Vector2i(35, 20)
name_min_size2 = Vector2i(35, 20)
fname = "Канал 3"
metadata/value0 = "SelfTest[1].SystemList[1].DevList[2].TestedParamList[0]['CurrentValue']"
metadata/value1 = "SelfTest[2].SystemList[1].DevList[2].TestedParamList[0]['CurrentValue']"
metadata/value2 = "SelfTest[0].SystemList[1].DevList[2]['TestPassed']"
metadata/state = ["SelfTest[0].SystemList[1].DevList[2]['TestPassed']"]

[node name="kanal4" parent="konverter/grid" instance=ExtResource("2_dmhrm")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Канал №4 конвертера 1000...6000 МГц"
value0 = 24.0
value1 = 27.0
min_value0 = 10.0
min_value1 = 15.0
max_value0 = 35.0
max_value1 = 30.0
step0 = 1.0
step1 = 1.0
value_name0 = "t, °C"
value_name1 = "U, В"
value_name2 = "CAN"
name_min_size0 = Vector2i(35, 20)
name_min_size1 = Vector2i(35, 20)
name_min_size2 = Vector2i(35, 20)
fname = "Канал 4"
metadata/value0 = "SelfTest[1].SystemList[1].DevList[3].TestedParamList[0]['CurrentValue']"
metadata/value1 = "SelfTest[2].SystemList[1].DevList[3].TestedParamList[0]['CurrentValue']"
metadata/value2 = "SelfTest[0].SystemList[1].DevList[3]['TestPassed']"
metadata/state = ["SelfTest[0].SystemList[1].DevList[3]['TestPassed']"]

[node name="kanal5" parent="konverter/grid" instance=ExtResource("2_dmhrm")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Канал №5 конвертера 1000...6000 МГц"
value0 = 24.0
value1 = 27.0
min_value0 = 10.0
min_value1 = 15.0
max_value0 = 35.0
max_value1 = 30.0
step0 = 1.0
step1 = 1.0
value_name0 = "t, °C"
value_name1 = "U, В"
value_name2 = "CAN"
name_min_size0 = Vector2i(35, 20)
name_min_size1 = Vector2i(35, 20)
name_min_size2 = Vector2i(35, 20)
fname = "Канал 5"
metadata/value0 = "SelfTest[1].SystemList[1].DevList[4].TestedParamList[0]['CurrentValue']"
metadata/value1 = "SelfTest[2].SystemList[1].DevList[4].TestedParamList[0]['CurrentValue']"
metadata/value2 = "SelfTest[0].SystemList[1].DevList[4]['TestPassed']"
metadata/state = ["SelfTest[0].SystemList[1].DevList[4]['TestPassed']"]

[node name="kanal6" parent="konverter/grid" instance=ExtResource("2_dmhrm")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Канал №6 конвертера 1000...6000 МГц"
value0 = 24.0
value1 = 27.0
min_value0 = 10.0
min_value1 = 15.0
max_value0 = 35.0
max_value1 = 30.0
step0 = 1.0
step1 = 1.0
value_name0 = "t, °C"
value_name1 = "U, В"
value_name2 = "CAN"
name_min_size0 = Vector2i(35, 20)
name_min_size1 = Vector2i(35, 20)
name_min_size2 = Vector2i(35, 20)
fname = "Канал 6"
metadata/value0 = "SelfTest[1].SystemList[1].DevList[5].TestedParamList[0]['CurrentValue']"
metadata/value1 = "SelfTest[2].SystemList[1].DevList[5].TestedParamList[0]['CurrentValue']"
metadata/value2 = "SelfTest[0].SystemList[1].DevList[5]['TestPassed']"
metadata/state = ["SelfTest[0].SystemList[1].DevList[5]['TestPassed']"]

[node name="kanal7" parent="konverter/grid" instance=ExtResource("2_dmhrm")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Канал №7 конвертера 1000...6000 МГц"
value0 = 24.0
value1 = 27.0
min_value0 = 10.0
min_value1 = 15.0
max_value0 = 35.0
max_value1 = 30.0
step0 = 1.0
step1 = 1.0
value_name0 = "t, °C"
value_name1 = "U, В"
value_name2 = "CAN"
name_min_size0 = Vector2i(35, 20)
name_min_size1 = Vector2i(35, 20)
name_min_size2 = Vector2i(35, 20)
fname = "Канал 7"
metadata/value0 = "SelfTest[1].SystemList[1].DevList[6].TestedParamList[0]['CurrentValue']"
metadata/value1 = "SelfTest[2].SystemList[1].DevList[6].TestedParamList[0]['CurrentValue']"
metadata/value2 = "SelfTest[0].SystemList[1].DevList[6]['TestPassed']"
metadata/state = ["SelfTest[0].SystemList[1].DevList[6]['TestPassed']"]

[node name="kanal8" parent="konverter/grid" instance=ExtResource("2_dmhrm")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Канал №8 конвертера 1000...6000 МГц"
value0 = 24.0
value1 = 27.0
min_value0 = 10.0
min_value1 = 15.0
max_value0 = 35.0
max_value1 = 30.0
step0 = 1.0
step1 = 1.0
value_name0 = "t, °C"
value_name1 = "U, В"
value_name2 = "CAN"
name_min_size0 = Vector2i(35, 20)
name_min_size1 = Vector2i(35, 20)
name_min_size2 = Vector2i(35, 20)
fname = "Канал 8"
metadata/value0 = "SelfTest[1].SystemList[1].DevList[7].TestedParamList[0]['CurrentValue']"
metadata/value1 = "SelfTest[2].SystemList[1].DevList[7].TestedParamList[0]['CurrentValue']"
metadata/value2 = "SelfTest[0].SystemList[1].DevList[7]['TestPassed']"
metadata/state = ["SelfTest[0].SystemList[1].DevList[7]['TestPassed']"]

[node name="antenna1" type="NinePatchRect" parent="."]
layout_mode = 0
offset_top = 115.0
offset_right = 580.0
offset_bottom = 521.0
texture = ExtResource("1_pfrxy")
patch_margin_left = 16
patch_margin_top = 16
patch_margin_right = 16
patch_margin_bottom = 16

[node name="lbl_fname" type="Label" parent="antenna1"]
self_modulate = Color(1, 1, 1, 0.62)
layout_mode = 0
offset_left = 5.0
offset_top = 5.0
offset_right = 575.0
offset_bottom = 25.0
text = "Антенна 400...1000 МГц"
horizontal_alignment = 1
vertical_alignment = 1

[node name="grid" type="GridContainer" parent="antenna1"]
layout_mode = 2
offset_left = 10.0
offset_top = 25.0
offset_right = 570.0
offset_bottom = 397.0
columns = 4

[node name="yelement1" parent="antenna1/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №1 диапазона 400...1000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 1"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[0].DevList[0].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[0].DevList[0].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[0].DevList[0]['TestPassed']"]

[node name="yelement2" parent="antenna1/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №2 диапазона 400...1000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 2"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[0].DevList[1].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[0].DevList[1].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[0].DevList[1]['TestPassed']"]

[node name="yelement3" parent="antenna1/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №3 диапазона 400...1000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 3"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[0].DevList[2].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[0].DevList[2].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[0].DevList[2]['TestPassed']"]

[node name="yelement4" parent="antenna1/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №4 диапазона 400...1000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 4"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[0].DevList[3].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[0].DevList[3].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[0].DevList[3]['TestPassed']"]

[node name="yelement5" parent="antenna1/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №5 диапазона 400...1000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 5"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[0].DevList[4].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[0].DevList[4].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[0].DevList[4]['TestPassed']"]

[node name="yelement6" parent="antenna1/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №6 диапазона 400...1000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 6"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[0].DevList[5].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[0].DevList[5].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[0].DevList[5]['TestPassed']"]

[node name="yelement7" parent="antenna1/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №7 диапазона 400...1000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 7"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[0].DevList[6].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[0].DevList[6].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[0].DevList[6]['TestPassed']"]

[node name="yelement8" parent="antenna1/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №8 диапазона 400...1000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 8"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[0].DevList[7].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[0].DevList[7].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[0].DevList[7]['TestPassed']"]

[node name="yelement9" parent="antenna1/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №9 диапазона 400...1000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 9"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[0].DevList[8].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[0].DevList[8].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[0].DevList[8]['TestPassed']"]

[node name="yelement10" parent="antenna1/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №10 диапазона 400...1000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 10"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[0].DevList[9].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[0].DevList[9].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[0].DevList[9]['TestPassed']"]

[node name="yelement11" parent="antenna1/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №11 диапазона 400...1000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 11"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[0].DevList[10].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[0].DevList[10].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[0].DevList[10]['TestPassed']"]

[node name="yelement12" parent="antenna1/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №12 диапазона 400...1000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 12"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[0].DevList[11].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[0].DevList[11].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[0].DevList[11]['TestPassed']"]

[node name="yelement13" parent="antenna1/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №13 диапазона 400...1000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 13"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[0].DevList[12].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[0].DevList[12].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[0].DevList[12]['TestPassed']"]

[node name="yelement14" parent="antenna1/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №14 диапазона 400...1000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 14"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[0].DevList[13].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[0].DevList[13].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[0].DevList[13]['TestPassed']"]

[node name="yelement15" parent="antenna1/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №15 диапазона 400...1000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 15"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[0].DevList[14].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[0].DevList[14].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[0].DevList[14]['TestPassed']"]

[node name="yelement16" parent="antenna1/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №16 диапазона 400...1000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 16"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[0].DevList[15].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[0].DevList[15].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[0].DevList[15]['TestPassed']"]

[node name="antenna2" type="NinePatchRect" parent="."]
layout_mode = 0
offset_top = 521.0
offset_right = 580.0
offset_bottom = 926.0
texture = ExtResource("1_pfrxy")
patch_margin_left = 16
patch_margin_top = 16
patch_margin_right = 16
patch_margin_bottom = 16

[node name="lbl_fname" type="Label" parent="antenna2"]
self_modulate = Color(1, 1, 1, 0.62)
layout_mode = 0
offset_left = 5.0
offset_top = 5.0
offset_right = 575.0
offset_bottom = 25.0
text = "Антенна 1000...6000 МГц"
horizontal_alignment = 1
vertical_alignment = 1

[node name="grid" type="GridContainer" parent="antenna2"]
layout_mode = 2
offset_left = 10.0
offset_top = 25.0
offset_right = 570.0
offset_bottom = 397.0
columns = 4

[node name="yelement1" parent="antenna2/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №1 диапазона 1000...6000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 1"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[1].DevList[0].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[1].DevList[0].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[1].DevList[0]['TestPassed']"]

[node name="yelement2" parent="antenna2/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №2 диапазона 1000...6000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 2"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[1].DevList[1].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[1].DevList[1].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[1].DevList[1]['TestPassed']"]

[node name="yelement3" parent="antenna2/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №3 диапазона 1000...6000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 3"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[1].DevList[2].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[1].DevList[2].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[1].DevList[2]['TestPassed']"]

[node name="yelement4" parent="antenna2/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №4 диапазона 1000...6000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 4"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[1].DevList[3].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[1].DevList[3].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[1].DevList[3]['TestPassed']"]

[node name="yelement5" parent="antenna2/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №5 диапазона 1000...6000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 5"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[1].DevList[4].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[1].DevList[4].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[1].DevList[4]['TestPassed']"]

[node name="yelement6" parent="antenna2/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №6 диапазона 1000...6000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 6"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[1].DevList[5].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[1].DevList[5].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[1].DevList[5]['TestPassed']"]

[node name="yelement7" parent="antenna2/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №8 диапазона 1000...6000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 7"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[1].DevList[6].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[1].DevList[6].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[1].DevList[6]['TestPassed']"]

[node name="yelement8" parent="antenna2/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №8 диапазона 1000...6000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 8"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[1].DevList[7].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[1].DevList[7].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[1].DevList[7]['TestPassed']"]

[node name="yelement9" parent="antenna2/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №9 диапазона 1000...6000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 9"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[1].DevList[8].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[1].DevList[8].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[1].DevList[8]['TestPassed']"]

[node name="yelement10" parent="antenna2/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №10 диапазона 1000...6000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 10"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[1].DevList[9].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[1].DevList[9].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[1].DevList[9]['TestPassed']"]

[node name="yelement11" parent="antenna2/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №11 диапазона 1000...6000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 11"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[1].DevList[10].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[1].DevList[10].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[1].DevList[10]['TestPassed']"]

[node name="yelement12" parent="antenna2/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №12 диапазона 1000...6000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 12"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[1].DevList[11].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[1].DevList[11].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[1].DevList[11]['TestPassed']"]

[node name="yelement13" parent="antenna2/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №13 диапазона 1000...6000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 13"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[1].DevList[12].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[1].DevList[12].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[1].DevList[12]['TestPassed']"]

[node name="yelement14" parent="antenna2/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №14 диапазона 1000...6000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 14"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[1].DevList[13].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[1].DevList[13].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[1].DevList[13]['TestPassed']"]

[node name="yelement15" parent="antenna2/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №15 диапазона 1000...6000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 15"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[1].DevList[14].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[1].DevList[14].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[1].DevList[14]['TestPassed']"]

[node name="yelement16" parent="antenna2/grid" instance=ExtResource("3_5ikxk")]
layout_mode = 2
size_flags_horizontal = 7
size_flags_vertical = 7
tooltip_text = "Антенный элемент №16 диапазона 1000...6000 МГц"
min_value0 = 10.0
max_value0 = 15.0
max_value1 = 10.0
value_name0 = "А"
value_name1 = "φ"
fname = "Элемент 16"
metadata/value0 = "SelfTest[1].SystemList[0].SystemList[1].DevList[15].TestedParamList[1]['CurrentValue']"
metadata/value1 = "SelfTest[1].SystemList[0].SystemList[1].DevList[15].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[1].SystemList[0].SystemList[1].DevList[15]['TestPassed']"]

[node name="adc" parent="." instance=ExtResource("4_mtf2n")]
layout_mode = 0
offset_left = 380.0
offset_top = 60.0
offset_right = 580.0
offset_bottom = 115.0
tooltip_text = "Плата АЦП ADCS500"
fname = "АЦП"
metadata/state = ["SelfTest[4].SystemList[0].DevList[1]['TestPassed']"]

[node name="dsp" parent="." instance=ExtResource("4_mtf2n")]
layout_mode = 0
offset_left = 380.0
offset_right = 580.0
offset_bottom = 60.0
tooltip_text = "Плата цифровой обработки сигналов BPL"
fname = "Сигн. проц."
metadata/state = ["SelfTest[4].SystemList[0].DevList[0]['TestPassed']"]

[node name="gen" parent="." instance=ExtResource("2_dmhrm")]
layout_mode = 2
offset_right = 145.0
offset_bottom = 115.0
tooltip_text = "Тестовый генератор"
min_value0 = -45.0
min_value1 = 20.0
max_value0 = 60.0
max_value1 = 30.0
value_name0 = "t, °C"
value_name1 = "U, В"
value_name2 = "CAN"
name_min_size0 = Vector2i(35, 20)
name_min_size1 = Vector2i(35, 20)
name_min_size2 = Vector2i(35, 20)
fname = "Генератор"
metadata/value0 = "SelfTest[1].SystemList[2].DevList[0].TestedParamList[0]['CurrentValue']"
metadata/value1 = "SelfTest[2].SystemList[2].DevList[0].TestedParamList[0]['CurrentValue']"
metadata/state = ["SelfTest[0].SystemList[2].DevList[0]['TestPassed']"]

[node name="rpu" parent="." instance=ExtResource("2_dmhrm")]
layout_mode = 2
offset_left = 145.0
offset_right = 380.0
offset_bottom = 115.0
tooltip_text = "Восьмиканальное прёмное устройство 20 ...1000 МГц"
min_value0 = 10.0
min_value1 = 5.0
max_value0 = 35.0
max_value1 = 20.0
value_name0 = "t, °C"
value_name1 = "U, В"
value_name2 = "CAN"
name_min_size0 = Vector2i(35, 20)
name_min_size1 = Vector2i(35, 20)
name_min_size2 = Vector2i(35, 20)
fname = "Приёмник 20...1000 МГц"
metadata/value0 = "SelfTest[1].SystemList[0].DevList[0]['TestPassed']"
metadata/value1 = "SelfTest[2].SystemList[0].DevList[0]['TestPassed']"
metadata/state = ["SelfTest[0].SystemList[0].DevList[3]['TestPassed']"]

[connection signal="pressed" from="konverter/grid/kanal1" to="." method="_on_item_pressed"]
[connection signal="pressed" from="konverter/grid/kanal2" to="." method="_on_item_pressed"]
[connection signal="pressed" from="konverter/grid/kanal3" to="." method="_on_item_pressed"]
[connection signal="pressed" from="konverter/grid/kanal4" to="." method="_on_item_pressed"]
[connection signal="pressed" from="konverter/grid/kanal5" to="." method="_on_item_pressed"]
[connection signal="pressed" from="konverter/grid/kanal6" to="." method="_on_item_pressed"]
[connection signal="pressed" from="konverter/grid/kanal7" to="." method="_on_item_pressed"]
[connection signal="pressed" from="konverter/grid/kanal8" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna1/grid/yelement1" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna1/grid/yelement2" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna1/grid/yelement3" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna1/grid/yelement4" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna1/grid/yelement5" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna1/grid/yelement6" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna1/grid/yelement7" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna1/grid/yelement8" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna1/grid/yelement9" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna1/grid/yelement10" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna1/grid/yelement11" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna1/grid/yelement12" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna1/grid/yelement13" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna1/grid/yelement14" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna1/grid/yelement15" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna1/grid/yelement16" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna2/grid/yelement1" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna2/grid/yelement2" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna2/grid/yelement3" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna2/grid/yelement4" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna2/grid/yelement5" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna2/grid/yelement6" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna2/grid/yelement7" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna2/grid/yelement8" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna2/grid/yelement9" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna2/grid/yelement10" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna2/grid/yelement11" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna2/grid/yelement12" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna2/grid/yelement13" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna2/grid/yelement14" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna2/grid/yelement15" to="." method="_on_item_pressed"]
[connection signal="pressed" from="antenna2/grid/yelement16" to="." method="_on_item_pressed"]
[connection signal="pressed" from="adc" to="." method="_on_item_pressed"]
[connection signal="pressed" from="dsp" to="." method="_on_item_pressed"]
[connection signal="pressed" from="gen" to="." method="_on_item_pressed"]
[connection signal="pressed" from="rpu" to="." method="_on_item_pressed"]
